NETCALL (Sub Commands) :
 xxxxxx-9 
17 Commands #2: NETCALL
The NETCALL is the callsign of the K-Net node The NETCALL must be entered before the
K-Net can be operational and must be different from any other callsign-SSID used in the
KPC-3 Plus. Entering or changing the NETCALL will cause a soft reset as memory is reallocated.